# [REGISTRY]

<- Property Sheets This sheet specifies which parameter is read or not read from the Registry when start-up. (cf. Parameters.)
When this sheet is selected first in the property sheets, the parameters marked with + in the list box are automatically read in mode at present. (In default, all the parameters is read automatically when start-up.)
[Auto Load] Adds + mark to the selected parameter in the list box in [REGISTRY]. Marked parameters will be read from Registory when start-up.
[Ignore] Removes + mark from the selected parameter in the list box. Unmarked parameters will not be read from Registory when start-up.
[All Set] in [REGISTRY] Adds + to all the parameters in the list box.
[All Clear] in [REGISTRY] Removes + from all the parameters in the list box.
Note: The automatic reading of the parameters set here become effective after the [Save] button on this sheet is pressed. Pressing the [Restore] button on this sheet shows the list of parameters to be read automatically with +.
[Save] in [REGISTRY] The settings are saved at the locations for the current mode of the Registry. The values of the parameters marked by + are automatically read when the start-up mode is the current mode.
[Restore] in [REGISTRY] The list of parameters to be read at start-up is obtained based on the current mode of the Registry and indicated with + set to the parameters displayed in the list box.
When the current setting is changed, the current settings are first obtained by this button. They can be corrected and saved.
Note: The [Apply] and [OK] buttons are unrelated to the settings in the [REGISTRY] sheet.
-------- Selected mode ----------
Default mode: specifies the start-up mode. The parameters specified for automatic reading for this mode are read in from the Registry at start-up. (The settings become effective after the [Save] button is pressed.)
Current mode: changes the current mode. This is reflected to the current dviout (you don't need to press the [Apply] or [OK] button.).
[Save] and [Restore] to the Registry of the various parameter values on each page of the property sheets are applied to the current mode in the Registry.
Current Print: When dviout is in the current mode set above, the mode can change to the mode set here only when Printing. (This becomes effective after the [Save] button is pressed.)
For example, you might want to employ different dpi when printing from when previewing (cf. Q_P6) or invoke Ghostscript to interpret PostScript \specials only when printing.
By specifying a mode in Current Print, such a temporal switching of mode is possible. However, when invoking an external application program such as dviprt, this setting is ignored.
Current Name: You can give a name to the current mode and this would make it easy to remember which mode has which specification. The name is displayed in the dialog for changing the mode by "Option -> Mode".