# Image data file

dviout can read image data files in the PS/EPS, WMF/EMF, raw PBM, BMP/BMC (monochrome, 16 colors, 256 colors, 65,535 colors, full color) formats and many other formats.
dviout can also handle the gzipped files transformed from the original image data files.
One can use Embedding into DVI file or the files must be placed in either the directory containing the dvi file or the directory specified by -gdat:.
See "Image data file specials".
For viewing these Image data files, checks the item Ghostscript under "Property Sheets->[Graphic]" as On (-GS:).
If you want to handle PostScript files, you need Ghostscript which supports the raw PBM output specified by -GIF: or the BMP output (corresponding to multiple colors). Then, specify the full path name in -gsx: (or press the button to open the executable file).
To read an image data file whose format is different from PS/EPS, WMF/EMF, raw PBM and BMP/BMC, the corresponding Susie plug-in (cf. -spi:) is required.