# Adjusting the Print Position

0. Print out some auxiliary dvi file (for example, test_org.dvi), then check the printed position on the paper. If the horizontal and vertical positions need to be adjusted, do the followings.
1. Select "Option -> Setup Parameters ->[Printer]" (see [Help]).
2. Uncheck the box of "Use default area for system drive" and press [OK]. Next, print out the auxiliary dvi file again and measure the length that should be corrected.
3. Again, select "Option -> Setup Parameters ->[Printer]" to set the length of the horizontal position that should be corrected in -LM: and the length of the vertical position that should be corrected in -TM: in units of 1/100 cm. (51 means 5.1 mm.)
Initially, both are zero and probably the actual printed position would be offset down and to the right. Then input these offset widths. Increasing -LM: makes the print position move to the left, and increasing -TM: makes it move up.
If you want to print out in the landscape orientation, first you should check the offsets by print out, for example, test_org.dvi in the landscape orientation. Then, (press the [Setup] button in the print dialog to make the printing direction horizontal.) specify the offset values in -RM: and -BM: for the vertical and horizontal direction, respectively.
4. Press [Save] to register to the Registry which is referred in the next dviout session (cf. Q_S1).
5. Press [Apply] to reflect the settings to the current session of the dviout.
Note: The printing position adjustment only for the temporary should be done by specifying -OX: and -OY:.