<p>
You need to transport <em>{good2}</em> from {f2} to {f3} in <em>{cy1}</em>.
</p>
<p>
{tx} Select <em>'{tool2}'</em> from the toolbar and choose the track tool to connect the two points between {w1} and {w2}.
</p>
<p>
<st>Connect the track here:</st> {cbor}.
</p>
