lwIP 2.2.1 Lightweight IP stack

System initialization

A truly complete and generic sequence for initializing the lwIP stack cannot be given because it depends on additional initializations for your runtime environment (e.g. timers).

We can give you some idea on how to proceed when using the raw API. We assume a configuration using a single Ethernet netif and the UDP and TCP transport layers, IPv4 and the DHCP client.

Call these functions in the order of appearance:

- lwip_init(): Initialize the lwIP stack and all of its subsystems.

- netif_add(struct netif *netif, ...): Adds your network interface to the netif_list. Allocate a struct netif and pass a pointer to this structure as the first argument. Give pointers to cleared ip_addr structures when using DHCP, or fill them with sane numbers otherwise. The state pointer may be NULL.

  The init function pointer must point to a initialization function for your Ethernet netif interface. The following code illustrates its use.

err_t netif_if_init(struct netif *netif)
{
u8_t i;
for (i = 0; i < ETHARP_HWADDR_LEN; i++) {
netif->hwaddr[i] = some_eth_addr[i];
}
init_my_eth_device();
return ERR_OK;
}

For Ethernet drivers, the input function pointer must point to the lwIP function ethernet_input() declared in "netif/etharp.h". Other drivers must use ip_input() declared in "lwip/ip.h".

- netif_set_default(struct netif *netif) Registers the default network interface.
- netif_set_link_up(struct netif *netif) This is the hardware link state; e.g. whether cable is plugged for wired Ethernet interface. This function must be called even if you don't know the current state. Having link up and link down events is optional but DHCP and IPv6 discover benefit well from those events.
- netif_set_up(struct netif *netif) This is the administrative (= software) state of the netif, when the netif is fully configured this function must be called.
- dhcp_start(struct netif *netif) Creates a new DHCP client for this interface on the first call. You can peek in the netif->dhcp struct for the actual DHCP status.
- sys_check_timeouts() When the system is running, you have to periodically call sys_check_timeouts() which will handle all timers for all protocols in the stack; add this to your main loop or equivalent.

netif::hwaddr
u8_t hwaddr[6U]
Definition: netif.h:350
netif
Definition: netif.h:269
ERR_OK
@ ERR_OK
Definition: err.h:55
err_t
s8_t err_t
Definition: err.h:96