# [Control] menu

Reset terminal
  Resets various terminal modes.
Are you there
  Sends a AYT (Are You There) telnet signal. Usually, the host sends back some message responding to it. This command is available only with a telnet connection.
Send break
  Sends a break signal to the host. Refer to sendbreak macro command.
Reset port
  Resets the serial port. This command is available only with a serial connection.
Broadcast command
  Display the dialog for the transmission of broadcast command.
Open TEK
  Opens the TEK window.
Close TEK
  Closes the TEK window.
Macro
  Runs a macro file.
Show Macro Window
  Shows the running macro window.