* add extra RTC, TIMER
* assert size constraints on TIMER
* clarify write-buffer for events handling
   https://devzone.nordicsemi.com/question/86564/nrf52-write-buffer/
* implement pin-reset, swo trace, trace pin configuration
* implement errata (see system_nrf52.c)
* check GPIO DETECTMODE and LATCH
