"eFM8"  - Fujitsu FM-8
								10/3/2016

--- Internal ROM image

    Main SYSTEM:
	BOOT_BAS8.ROM    $FE00 - $FFFF BOOT ROM(Basic Mode)
	BOOT_DOS8.ROM    $FE00 - $FFFF BOOT ROM(Dos Mode)
	BOOT_BBL8.ROM    $FE00 - $FFFF BOOT ROM(Bubble casette Mode / optional)
	BOOT_1MB.ROM	 $FE00 - $FFFF BOOT ROM(8" Floppy Mode / optional)
	
	FBASIC10.ROM	$8000 - $FBFF F-BASIC V1.0

    Sub System:
	SUBSYS_8.ROM    $D800 - $FFFF Subsystem monitor and font.

    Optional:
	Please select one of two:
	KANJI1.ROM      JIS class 1 Kanji ROM $20000 bytes
	KANJI.ROM       JIS class 1 Kanji ROM $20000 bytes
	FDDSEEK.WAV     Sound file of FDD SEEKING.
	RELAY_ON.WAV    Sound file of turning on a CMT's RELAY.	
	RELAYOFF.WAV    Sound file of turning off a CMT's RELAY.

--- Key maps

	Virtual		PC
	--------------------------------
	ESC		Kanji or Pause/Break
	BREAK		Esc
	Space		Muhenkan, Space and Henkan
	GRPH		Left ALT(Windows) or Left Windows key
	KANA		Katakana Hiragana
	INS		Insert
	DEL		Delete
	BS(⇐)		Back Space
	HOME		Home
	CLS		Page Down
	DUP		End
	EL		Page Up
	= (NUMPAD)	=	Scroll Lock(Windows) or Right Windows key
	Comma (NUMPAD)	Right Alt

	Anothe Keys include NUMPAD are refer to physical keyboard.
	
----------------------------------------
K.Ohta
whatisthis.sowhat@gmail.com
https://github.com/Artanejp/
Twitter @Artanejp

