"ePX-7" - PIONEER PX-7 emulator for Win32
								4/9/2014

--- Internal ROM image

	BASIC.ROM	$0000-$7FFF of SLOT 0
	EXT.ROM		$4000-$5FFF of SLOT 2

    Optional:
	RELAY_ON.WAV    Sound file of turning on a CMT's RELAY.	
	RELAYOFF.WAV    Sound file of turning off a CMT's RELAY.

--- Laser Disc images

	To use *,ogv image, you need to install the DirectShow filter.
	http://www.xiph.org/dshow/downloads/

	But this codec is very heavy, so I recommend to convert *.ogv images
	to *.avi format. (512x384, PCM 16bit Stereo)

	To use *.avi image, you need *.ini files that contains the frame info.
	*.ini files are in px7/ folder in this binary archive.

--- Key maps

	Virtual		PC
	--------------------------------
	SELECT		F9
	STOP		Pause

----------------------------------------
TAKEDA, toshiya
t-takeda@m1.interq.or.jp
http://homepage3.nifty.com/takeda-toshiya/
