H add serious PCM test application to test various period/buffer size
  combinations to determine possible problems in the lowlevel drivers
M think about xrun recovery helpers
L move OSS emulation to user space? (pseudo device driver and daemon)
