DIS PIXIT for the PTS tool.

PTS version: 6.1

* - different than PTS defaults
& - should be set to IUT Bluetooth address

		Required PIXIT settings
-------------------------------------------------------------------------------
Parameter Name						Value
-------------------------------------------------------------------------------
TSPX_bd_addr_iut					112233445566 (*&)
TSPX_time_guard						180000
TSPX_use_implicit_send					TRUE
TSPX_tester_database_file				C:/Program Files/...
TSPX_mtu_size						23
TSPX_secure_simple_pairing_pass_key_confirmation	FALSE
TSPX_delete_link_key					FALSE
TSPX_pin_code						0000
TSPX_use_dynamic_pin					FALSE
TSPX_delete_ltk						FALSE
TSPX_security_enabled					TRUE (*)
TSPX_iut_setup_att_over_br_edr				FALSE
TSPX_tester_appearance					0000
TSPX_iut_use_resolvable_random_address			FALSE
-------------------------------------------------------------------------------
