/*
 *  Copyright 2000-2011 Intel Corporation All Rights Reserved
 *
 * Permission is hereby granted, free of charge, to any person obtaining a
 * copy of this software and associated documentation files (the
 * "Software"), to deal in the Software without restriction, including
 * without limitation the rights to use, copy, modify, merge, publish,
 * distribute, sub license, and/or sell copies of the Software, and to
 * permit persons to whom the Software is furnished to do so, subject to
 * the following conditions:
 *
 * The above copyright notice and this permission notice (including the
 * next paragraph) shall be included in all copies or substantial portions
 * of the Software.
 *
 * THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS
 * OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF
 * MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NON-INFRINGEMENT.
 * IN NO EVENT SHALL PRECISION INSIGHT AND/OR ITS SUPPLIERS BE LIABLE FOR
 * ANY CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT,
 * TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION WITH THE
 * SOFTWARE OR THE USE OR OTHER DEALINGS IN THE SOFTWARE.
 *
 * This file was originally licensed under the following license
 *
 *  Licensed under the Apache License, Version 2.0 (the "License");
 *  you may not use this file except in compliance with the License.
 *  You may obtain a copy of the License at
 *
 *      http://www.apache.org/licenses/LICENSE-2.0
 *
 *  Unless required by applicable law or agreed to in writing, software
 *  distributed under the License is distributed on an "AS IS" BASIS,
 *  WITHOUT WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied.
 *  See the License for the specific language governing permissions and
 *  limitations under the License.
 */
//   42    // Total instruction count
//    1    // Total kernel count



// Module name: common.inc
//
// Common header file for all Video-Processing kernels
//

.default_execution_size (16)
.default_register_type  :ub

.reg_count_total        128
.reg_count_payload      7

//========== Common constants ==========


//========== Macros ==========


//Fast Jump, For more details see "Set_Layer_N.asm"


//========== Defines ====================

//========== Static Parameters (Common To All) ==========
//r1


//r2

                                    //  e.g.            byte0   byte1  byte2
                                    // YUYV               0       1      3
                                    // YVYU               0       3      1

//Color Pipe (IECP) parameters


//ByteCopy


//r4

                                    //  e.g.              byte0           byte1           byte2
                                    // YUYV                 0               1               3
                                    // YVYU                 0               3               1


//========== Inline parameters (Common To All) ===========


//============== Binding Index Table===========
//Common between DNDI and DNUV


//================= Common Message Descriptor =====
// Message descriptor for thread spawning
// Message Descriptors
//                = 000 0001 (min message len 1 ) 0,0000 (resp len 0   -add later)
//                  0000,0000,0000
//                  0001(Spawn a root thread),0001 (Root thread spawn thread)
//                = 0x02000011
// Thread Spawner Message Descriptor


// Message descriptor for atomic operation add
// Message Descriptors
//                = 000 0110 (min message len 6 ) 0,0000 (resp len 0   -add later)
//                  1(header present)001,10(typed atomic operation)0(return enabled)0(slot group, low 8 bits),0111 (AOP_Add)
//                  0000,0000 (Binding table index, added later)
//                = 0x02000011

// Atomic Operation Add Message Descriptor


// Message descriptor for dataport media write
        // Message Descriptors
                //                = 000 0001 (min message len 1 - add later) 00000 (resp len 0)
                //                  1 (header present 1) 0 1010 (media block write) 000000
                //                  00000000 (binding table index - set later)
                //                = 0x020A8000


// Message Length defines


// Response Length defines


// Block Width and Height Size defines


// Extended Message Descriptors


// Common message descriptors:


//===================== Math Function Control ===================================


//============ Message Registers ===============
                             // buf4 starts from r28


//#define mMSGHDR_EOT  r43    // Dummy Message Register for EOT


.declare    mubMSGPAYLOAD  Base=r30 ElementSize=1 SrcRegion=<16;16,1> Type=ub
.declare    muwMSGPAYLOAD  Base=r30 ElementSize=2 SrcRegion=<16;16,1> Type=uw
.declare    mudMSGPAYLOAD  Base=r30 ElementSize=4 SrcRegion=<8;8,1> Type=ud
.declare    mfMSGPAYLOAD   Base=r30 ElementSize=4 SrcRegion=<8;8,1> Type=f

//=================== End of thread instruction ===========================


//=====================Pointers Used=====================================


//=======================================================================


//r11-r17
// Define temp space for any usages


// Common Buffers


// temp space for rotation

.declare fROBUF		  Base=r11.0		ElementSize=4		SrcRegion=<8;8,1>		  DstRegion=<1>		Type=f

.declare udROBUF		Base=r11.0		ElementSize=4		SrcRegion=<8;8,1>		  DstRegion=<1>		Type=ud

.declare uwROBUF		Base=r11.0		ElementSize=2		SrcRegion=<16;16,1>		DstRegion=<1>		Type=uw

.declare ubROBUF		Base=r11.0		ElementSize=1		SrcRegion=<16;16,1>		DstRegion=<1>		Type=ub

.declare ub4ROBUF 	Base=r11.0		ElementSize=1		SrcRegion=<32;8,4>		DstRegion=<4>		Type=ub


// End of common.inc


// FileName:		PL2_AVS_Buf_3.asm
// Author:			Tatiya, Rupesh
// Description:		Loads 8x8 AVS/IEF PL2 data into Buffer 0



// FileName     :   PL2_AVS_Buf.asm
// Author       :   Tatiya, Rupesh
// Description  :   Loads 8x8 AVS/IEF PL2 data into Buffer N



// Module name: Scaling.inc




// Description: Includes all definitions explicit to Fast Composite.




// End of common.inc


//========== GRF partition ==========
     // r0 header            :   r0          (1 GRF)
     // Static parameters    :   r1 - r6     (6 GRFS)
     // Inline parameters    :   r7 - r8     (2 GRFs)
     // MSGSRC               :   r27         (1 GRF)
//===================================

//Interface:
//========== Static Parameters (Explicit To Fast Composite) ==========
//r1
//CSC Set 0


.declare udCSC_CURBE    Base=r1.0      ElementSize=4       Type=ud

//Constant alpha


//r2


// Gen7 AVS WA


// WiDi Definitions


//Colorfill


                                      // 0: 0-degree, 1: 90, 2: 180, 3: 270-degree, clockwise.	    

.declare ubCOLOR_PIXEL_VAL      Base=r2.20      ElementSize=1       SrcRegion=<0;1,0>       DstRegion=<1>       Type=ub

//r3
//Normalised Ratio of Horizontal step size with main video for all layers


    //Normalised Ratio of Horizontal step size with main video for all layers becomes
    //Normalised Horizontal step size for all layers in VP_Setup.asm


//r4
//Normalised Vertical step size for all layers


//r5
//Normalised Vertical Frame Origin for all layers


//r6
//Normalised Horizontal Frame Origin for all layers


//========== Inline Parameters (Explicit To Fast Composite) ==========


//Main video Step X


//====================== Binding table (Explicit To Fast Composite)=========================================


//Used by Interlaced Scaling Kernels


//========== Sampler State Table Index (Explicit To Fast Composite)==========
//Sampler Index for AVS/IEF messages


//Sampler Index for SIMD16 sampler messages


//=============================================================================

.declare fBUFFER_0      Base=r64.0       ElementSize=4       SrcRegion=<8;8,1>       DstRegion=<1>       Type=f
.declare fBUFFER_1      Base=r80.0       ElementSize=4       SrcRegion=<8;8,1>       DstRegion=<1>       Type=f
.declare fBUFFER_2      Base=r96.0       ElementSize=4       SrcRegion=<8;8,1>       DstRegion=<1>       Type=f
.declare fBUFFER_3      Base=r112.0       ElementSize=4       SrcRegion=<8;8,1>       DstRegion=<1>       Type=f
.declare fBUFFER_4      Base=r28.0       ElementSize=4       SrcRegion=<8;8,1>       DstRegion=<1>       Type=f
.declare fBUFFER_5      Base=r46.0       ElementSize=4       SrcRegion=<8;8,1>       DstRegion=<1>       Type=f

.declare udBUFFER_0     Base=r64.0       ElementSize=4       SrcRegion=<8;8,1>       DstRegion=<1>       Type=ud
.declare udBUFFER_1     Base=r80.0       ElementSize=4       SrcRegion=<8;8,1>       DstRegion=<1>       Type=ud
.declare udBUFFER_2     Base=r96.0       ElementSize=4       SrcRegion=<8;8,1>       DstRegion=<1>       Type=ud
.declare udBUFFER_3     Base=r112.0       ElementSize=4       SrcRegion=<8;8,1>       DstRegion=<1>       Type=ud
.declare udBUFFER_4     Base=r28.0       ElementSize=4       SrcRegion=<8;8,1>       DstRegion=<1>       Type=ud
.declare udBUFFER_5     Base=r46.0       ElementSize=4       SrcRegion=<8;8,1>       DstRegion=<1>       Type=ud

.declare uwBUFFER_0     Base=r64.0       ElementSize=2       SrcRegion=<16;16,1>     DstRegion=<1>       Type=uw
.declare uwBUFFER_1     Base=r80.0       ElementSize=2       SrcRegion=<16;16,1>     DstRegion=<1>       Type=uw
.declare uwBUFFER_2     Base=r96.0       ElementSize=2       SrcRegion=<16;16,1>     DstRegion=<1>       Type=uw
.declare uwBUFFER_3     Base=r112.0       ElementSize=2       SrcRegion=<16;16,1>     DstRegion=<1>       Type=uw
.declare uwBUFFER_4     Base=r28.0       ElementSize=2       SrcRegion=<16;16,1>     DstRegion=<1>       Type=uw
.declare uwBUFFER_5     Base=r46.0       ElementSize=2       SrcRegion=<16;16,1>     DstRegion=<1>       Type=uw

.declare ubBUFFER_0     Base=r64.0       ElementSize=1       SrcRegion=<16;16,1>     DstRegion=<1>       Type=ub
.declare ubBUFFER_1     Base=r80.0       ElementSize=1       SrcRegion=<16;16,1>     DstRegion=<1>       Type=ub
.declare ubBUFFER_2     Base=r96.0       ElementSize=1       SrcRegion=<16;16,1>     DstRegion=<1>       Type=ub
.declare ubBUFFER_3     Base=r112.0       ElementSize=1       SrcRegion=<16;16,1>     DstRegion=<1>       Type=ub
.declare ubBUFFER_4     Base=r28.0       ElementSize=1       SrcRegion=<16;16,1>     DstRegion=<1>       Type=ub
.declare ubBUFFER_5     Base=r46.0       ElementSize=1       SrcRegion=<16;16,1>     DstRegion=<1>       Type=ub

.declare ub4BUFFER_0    Base=r64.0       ElementSize=1       SrcRegion=<32;8,4>      DstRegion=<4>       Type=ub
.declare ub4BUFFER_1    Base=r80.0       ElementSize=1       SrcRegion=<32;8,4>      DstRegion=<4>       Type=ub
.declare ub4BUFFER_2    Base=r96.0       ElementSize=1       SrcRegion=<32;8,4>      DstRegion=<4>       Type=ub
.declare ub4BUFFER_3    Base=r112.0       ElementSize=1       SrcRegion=<32;8,4>      DstRegion=<4>       Type=ub
.declare ub4BUFFER_4    Base=r28.0       ElementSize=1       SrcRegion=<32;8,4>      DstRegion=<4>       Type=ub
.declare ub4BUFFER_5    Base=r46.0       ElementSize=1       SrcRegion=<32;8,4>      DstRegion=<4>       Type=ub

//Pointer to mask reg


//r18


//Always keep Cannel Pointers and Offsets in same GRF, so that we can use
// NODDCLR, NODDCHK flags. -rT


.declare udCSC_COEFF_0  Base=r18.0    ElementSize=4 Type=ud       // 1 GRF

//r19


.declare udCSC_COEFF_1  Base=r19.0    ElementSize=4 Type=ud       // 1 GRF


//r20

.declare uwALPHA_MASK_REG_TEMP  Base=r20.0    ElementSize=2 SrcRegion=<16;16,1> Type=uw        // 1 GRF

//r21

.declare uwALPHA_MASK_REG       Base=r21.0         ElementSize=2 SrcRegion=<16;16,1> Type=uw        // 1 GRF

//r22


//Always keep Cannel Pointers and Offsets in same GRF, so that we can use
// NODDCLR, NODDCHK flags. -rT


//Keep fORIGIN_X_NLAS, fY_OFFSET_2ND_BLOCK, fSTEP_X_NLAS, pMSGDSC_COPY, ubCONST_ALPHA_COPY as
//sub registers of same GRF to enable using NODDCLR NODDCHK. -rT

//r23


//Lumakey


//r24


//r25


//r26


//defines to generate LABELS during compile time.


        // Message Header
        // m0.7         31:0    Debug
        // m0.6         31:0    Debug
        // m0.5         31:0    Ignored
        // m0.4         31:0    Ignored
        // m0.3         31:0    Ignored
        // m0.2         31:16   Ignored
        //              15      Alpha Write Channel Mask        enable=0, disable=1
        //              14      Blue Write Channel Mask  (U)
        //              13      Green Write Channel Mask (Y)
        //              12      Red Write Channel Mask   (V)
        //              11:0    Ignored
        // m0.1                 Ignored
        // m0.0                 Ignored


        // AVS payload
        // m1.7                 Group ID Number
        // m1.6                 U 2nd Derivative        ---> NLAS dx
        // m1.5                 Delta V                 ---> Step Y
        // m1.4                 Delta U                 ---> Step X
        // m1.3                 Pixel 0 V Address       ---> ORIY (Y0)
        // m1.2                 Pixel 0 U Address       ---> ORIX (X0)
        // m1.1                 Vertical Block Number
        // m1.0                 Reserved

        // Sampler Message Descriptor
        // 31:29        Reserved                        000
        // 28:25        Message length                  0010
        // 24:20        Response length                 xxxxx   ---> 4GRFs for each enabled channel (AVS), 2GRFs for each enabled channel (sample unorm)
        // 19           Header Present                  1
        // 18:17        SIMD Mode                       11      ---> SIMD32/64
        // 16:12        Message Type                    xxxxx   ---> 01011 sample_8x8, 01100 (sample_unorm), 01010 (sample_unorm+killpix)
        // 11:8         Sampler Index                   xxxx
        // 7:0          Binding Table Index             xxxxxxxx


        // Msg Header M0.2
        // 15:15        Alpha Write Channel Mask, 0: written back, 1: not written back
        // 14:14        Blue  Write Channel Mask
        // 13:13        Green Write Channel Mask
        // 12:12        Red   Write Channel Mask


//By design, Buffer 0,1,2,3 always have Layer 0 and Buffer 4,5 always have L1-L7


//used to generate LABELS at compile time.


        // 18:17        SIMD Mode                       10      ---> SIMD16
        // 16:12        Message Type                    xxxxx   ---> 00000 (SIMD16)


//r10-17  - 8 GRFs to load SIMD16 data (upto 4 channels)
//r18-19  - 2 GRFs to store sampler ramp.

    .declare mfSCALING_0X_34X_PAYLOAD	Base=r14.0	ElementSize=4		SrcRegion=<8;8,1>		DstRegion=<1>		Type=f
    .declare muwSCALING_0X_34X_PAYLOAD	Base=r14.0	ElementSize=2		SrcRegion=<16;16,1>		DstRegion=<1>		Type=uw
    .declare mudCALING_0X_34X_PAYLOAD	Base=r14.0	ElementSize=4		SrcRegion=<8;8,1>		DstRegion=<1>		Type=ud
    .declare mubCALING_0X_34X_PAYLOAD	Base=r14.0	ElementSize=1		SrcRegion=<32;32,1>		DstRegion=<1>		Type=ub


	.declare fSCALING_0X_34X_TEMP		Base=r11.0	ElementSize=4		SrcRegion=<8;8,1>		DstRegion=<1>		Type=f
	.declare udSCALING_0X_34X_TEMP		Base=r11.0	ElementSize=4		SrcRegion=<8;8,1>		DstRegion=<1>		Type=ud
	.declare ub4SCALING_0X_34X_TEMP		Base=r11.0	ElementSize=1		SrcRegion=<32;8,4>		DstRegion=<1>		Type=ub
	.declare uwSCALING_0X_34X_TEMP		Base=r11.0	ElementSize=2		SrcRegion=<16;16,1>		DstRegion=<1>		Type=uw

	// Sampler ramp is used for Scaling 0X_0.34X
	.declare	fSAMPLER_RAMP  		Base=r11.0 ElementSize=4 SrcRegion=<8;8,1> Type=f		// 1 GRFs, 8 elements


	//#define rMSGDSC_UV    		r23.0


//End of _SCALING_


    //Check if layer is to be skipped


        // f0.1 pre-computed in Set_Layer_0
        (-f0.1)  jmpi  (1)  SKIP_AVS_LOAD_L0_3_


    //AVS_PAYLOAD already has all the data loaded at this point
    add (1)     a0.0:ud     r23.5<0;1,0>:ud      0x44EB400:ud      //msg desc

    mov (1)     r16.2:ud      0x0000D000:ud                                        // Enable Red channel


    // set the vertical block number


      add (1)   r25.1<1>:ud    r9.12:uw  3:ud


    mov (8)     r17.0:ud      r25.0<8;8,1>:ud                                     // Copy msg payload mirrors to MRFs

    // Gen7 AVS WA Only for YUV packed surfaces, NV12 and Y-channel only for Planar surfaces
    //   if (((int)(u_left*width + 5.0/256) > (int)(u_left*width)) 
    //   {
    //       modified_u_coord = u_coord – 5.0/(256*width); //floating point
    //   }
    //   else if(((int)(u_left*width + 255.0/256) == (int)(u_left*width)) 
    //   {
    //       modified_u_coord = u_coord + 1.0/(256*width); //floating point
    //   }
    //   else{
    //       modified_u_coord = u_coord;
    //   }
    //   Where u_left = u – 2*du + 3*ddu for IEF On
    //   And u_left = u for IEF Off case
    //   

    // check whether Gen7 AVS WA is enabled,
    mov  (1)    r14.8:uw            f0.0:uw                           // save f0.0
    mov  (1)    r14.5:f             r17.2<0;1,0>:f           // save pixel 0 U for chroma

    and.nz.f0.0  (1)     null<1>:uw     r2.3:uw    0x2:uw
    (-f0.0)jmpi  (1)     GEN7_PL2_AVS_WA_DONE_L0_3_

    // Gen7 AVS WA, check if IEF is ON for choosing Gen7 AVS WA formula

    and.nz.f0.0  (8)     null<1>:uw     r2.3<0;1,0>:uw             0x4:uw
    (f0.0)mov (8)    acc0.0:f          r17.2<0;1,0>:f
    (f0.0)mac (8)    acc0.0:f          r17.4<0;1,0>:f    -2.0:f
    (f0.0)mac (8)    acc0.0:f          r17.6<0;1,0>:f     3.0:f
    (f0.0)mov (1)    r14.2:f        acc0:f                                 // IEF ON,  rTEMP3.2 = u_left
    (-f0.0)mov (1)   r14.2:f        r17.2<0;1,0>:f                // IEF OFF, rTEMP3.2 = u_left

    and (1)         r14.1:ud     r2.3:uw    0xFFF8:uw
    asr (1)         r14.1:ud     r14.1:ud    3:d
    mov (1)         r14.1:f      r14.1:ud

    // Gen7 AVS WA, if (int)(u_left*width + 5.0/256) > (int)(u_left*width)
    mul (1)          r14.0:f        r14.2:f                  r14.1:f    // rTEMP3.0 = u_left*width
    add (1)          r14.2:f        r14.0:f                  0.01953125:f  // rTEMP3.2 = u_left*width + 5.0/256
    add (1)          r14.3:f        r14.0:f                  0.99609375:f  // rTEMP3.3 = u_left*width + 255.0/256

    //Check if the values are < 0 and account for (int) cast of negative numbers

    //(int)(u_left*width)
    cmp.l.f0.0 (1)   null<1>:f          r14.0:f                  0.00000000:f          
    mov (1)          r14.0:d        r14.0:f
    (f0.0)add (1)    r14.0:d        r14.0<0;1,0>:d           -1:d        

    //(int)(u_left*width + 5.0/256)
    cmp.l.f0.0 (1)   null<1>:f          r14.2:f                  0.00000000:f          
    mov (1)          r14.2:d        r14.2:f        
    (f0.0)add (1)    r14.2:d        r14.2<0;1,0>:d           -1:d        

    //(int)(u_left*width + 255.0/256)
    cmp.l.f0.0 (1)   null<1>:f          r14.3:f                  0.00000000:f          
    mov (1)          r14.3:d        r14.3:f
    (f0.0)add (1)    r14.3:d        r14.3<0;1,0>:d           -1:d        

    mov  (1)    f0.0:uw                0:uw                   // clear flag
    //if (((int)(u_left*width + 5.0/256) > (int)(u_left*width))
    cmp.g.f1.0  (1)     null<1>:d        r14.2:d    r14.0:d
    // modified_u_coord = u_coord – 5.0/(256*width); //floating point
    (f1.0) add (1)     r17.2:f       r17.2<0;1,0>:f   -r2.3:f
    //else if(((int)(u_left*width + 255.0/256) == (int)(u_left*width)) 
    (-f1.0) cmp.e.f0.0  (1) null<1>:d    r14.3:d    r14.0:d
    // modified_u_coord = u_coord + 1.0/(256*width); //floating point
    (f0.0) add (1)     r17.2:f       r17.2<0;1,0>:f   r2.2:f

GEN7_PL2_AVS_WA_DONE_L0_3_:
    mov  (1)    f0.0:uw                r14.8:uw                   // restore f0.0

    send (1)    uwBUFFER_3(0)<1>   r16    0x2    a0.0:ud
    // Returns Y data in 4 GRFs in scrambled order

    mov  (1)    r17.2:f       r14.5:f                    // restore pixel 0 U for chroma, No AVS WA for chroma

    add (1)     a0.0:ud                r23.5<0;1,0>:ud      0x48EB801:ud            // msg desc; 1 is added to change BI to UV
    mov (1)     r16.2:ud      0x0000A000:ud                                               // Enable Red+Blue channel

    send (1)    uwBUFFER_3(4)<1>   r16    0x2    a0.0:ud
    // Returns UV data in 8 GRFs in scrambled order

SKIP_AVS_LOAD_L0_3_:
    nop


