lwIP 2.2.1 Lightweight IP stack

Enumerations
iana.h File Reference

## Enumerations
enum | lwip_iana_hwtype { LWIP_IANA_HWTYPE_ETHERNET = 1 }
enum | lwip_iana_port_number { LWIP_IANA_PORT_SMTP = 25, LWIP_IANA_PORT_DHCP_SERVER = 67, LWIP_IANA_PORT_DHCP_CLIENT = 68, LWIP_IANA_PORT_TFTP = 69, LWIP_IANA_PORT_HTTP = 80, LWIP_IANA_PORT_SNTP = 123, LWIP_IANA_PORT_NETBIOS = 137, LWIP_IANA_PORT_SNMP = 161, LWIP_IANA_PORT_SNMP_TRAP = 162, LWIP_IANA_PORT_HTTPS = 443, LWIP_IANA_PORT_SMTPS = 465, LWIP_IANA_PORT_MQTT = 1883, LWIP_IANA_PORT_MDNS = 5353, LWIP_IANA_PORT_SECURE_MQTT = 8883 }

## Detailed Description

IANA assigned numbers (RFC 1700 and successors)