lwIP 2.2.1 Lightweight IP stack

Functions
TCP only
APIs » Sequential-style APIs » Netconn API

## Functions
err_t | netconn_listen_with_backlog (struct netconn *conn, u8_t backlog)
err_t | netconn_accept (struct netconn *conn, struct netconn **new_conn)
err_t | netconn_recv_tcp_pbuf (struct netconn *conn, struct pbuf **new_buf)
err_t | netconn_recv_tcp_pbuf_flags (struct netconn *conn, struct pbuf **new_buf, u8_t apiflags)
err_t | netconn_write_partly (struct netconn *conn, const void *dataptr, size_t size, u8_t apiflags, size_t *bytes_written)
err_t | netconn_close (struct netconn *conn)
err_t | netconn_shutdown (struct netconn *conn, u8_t shut_rx, u8_t shut_tx)

## Detailed Description

TCP only functions

## Function Documentation

## ◆ netconn_accept()

err_t netconn_accept | ( | struct netconn * | conn,
|  | struct netconn ** | new_conn
| ) |  |

Accept a new connection on a TCP listening netconn.

Parameters

  conn | the TCP listen netconn
  new_conn | pointer where the new connection is stored

Returns
  ERR_OK if a new connection has been received or an error code otherwise

## ◆ netconn_close()

err_t netconn_close | ( | struct netconn * | conn | ) |

Close a TCP netconn (doesn't delete it).

Parameters

  conn | the TCP netconn to close

Returns
  ERR_OK if the netconn was closed, any other err_t on error

## ◆ netconn_listen_with_backlog()

err_t netconn_listen_with_backlog | ( | struct netconn * | conn,
|  | u8_t | backlog
| ) |  |

Set a TCP netconn into listen mode

Parameters

  conn | the tcp netconn to set to listen mode
  backlog | the listen backlog, only used if TCP_LISTEN_BACKLOG==1

Returns
  ERR_OK if the netconn was set to listen (UDP and RAW netconns don't return any error (yet?))

## ◆ netconn_recv_tcp_pbuf()

err_t netconn_recv_tcp_pbuf | ( | struct netconn * | conn,
|  | struct pbuf ** | new_buf
| ) |  |

Receive data (in form of a pbuf) from a TCP netconn

Parameters

  conn | the netconn from which to receive data
  new_buf | pointer where a new pbuf is stored when received data

Returns
  ERR_OK if data has been received, an error code otherwise (timeout, memory error or another error,

See also
  netconn_recv_data) ERR_ARG if conn is not a TCP netconn

## ◆ netconn_recv_tcp_pbuf_flags()

err_t netconn_recv_tcp_pbuf_flags | ( | struct netconn * | conn,
|  | struct pbuf ** | new_buf,
|  | u8_t | apiflags
| ) |  |

Receive data (in form of a pbuf) from a TCP netconn

Parameters

  conn | the netconn from which to receive data
  new_buf | pointer where a new pbuf is stored when received data
  apiflags | flags that control function behaviour. For now only: NETCONN_DONTBLOCK: only read data that is available now, don't wait for more data

Returns
  ERR_OK if data has been received, an error code otherwise (timeout, memory error or another error,

See also
  netconn_recv_data) ERR_ARG if conn is not a TCP netconn

## ◆ netconn_shutdown()

err_t netconn_shutdown | ( | struct netconn * | conn,
|  | u8_t | shut_rx,
|  | u8_t | shut_tx
| ) |  |

Shut down one or both sides of a TCP netconn (doesn't delete it).

Parameters

  conn | the TCP netconn to shut down
  shut_rx | shut down the RX side (no more read possible after this)
  shut_tx | shut down the TX side (no more write possible after this)

Returns
  ERR_OK if the netconn was closed, any other err_t on error

## ◆ netconn_write_partly()

err_t netconn_write_partly | ( | struct netconn * | conn,
|  | const void * | dataptr,
|  | size_t | size,
|  | u8_t | apiflags,
|  | size_t * | bytes_written
| ) |  |

Send data over a TCP netconn.

Parameters

  conn | the TCP netconn over which to send data
  dataptr | pointer to the application buffer that contains the data to send
  size | size of the application data to send
  apiflags | combination of following flags : NETCONN_COPY: data will be copied into memory belonging to the stack NETCONN_MORE: for TCP connection, PSH flag will be set on last segment sent NETCONN_DONTBLOCK: only write the data if all data can be written at once
  bytes_written | pointer to a location that receives the number of written bytes

Returns
  ERR_OK if data was sent, any other err_t on error