
Argyll CMS README file - Version 1.5.0
--------------------------------------

Date: 8th March 2013   
Author: Graeme Gill

Introduction

ArgyllCMS is an ICC compatible color management system, available as Open Source.
It supports accurate ICC profile creation for scanners, cameras and film
recorders, and calibration and profiling of displays and RGB & CMYK printers.
Spectral sample data is supported, allowing a selection of illuminants observer
types, and paper fluorescent whitener additive compensation. Profiles can also
incorporate source specific gamut mappings for perceptual and saturation intents.
Gamut mapping and profile linking uses the CIECAM02 appearance model, a unique
gamut mapping algorithm, and a wide selection of rendering intents. Device Link
can be created with a wide variety of advanced options. It also includes code for
the fastest portable 8 bit raster color conversion engine available anywhere, as
well as support for fast, fully accurate 16 bit conversion. Device color gamuts
can also be viewed and compared using a VRML viewer. Comprehensive documentation
is provided for each major tool, and a general guide to using the tools for typical
color management tasks is also available. A mailing list provides support for
more advanced usage.

This is Version 1.5.1, a bug fix update to V1.5.0 released on 1st March 2013.
The first public release of icclib was in November 1998,
and of Argyll was in October 2000. Code development commenced in 1995. See
Changes Summary for an overview of changes since the last release. Changes
between revisions is detailed in the log.txt file that accompanies the source code. 

It is licensed under the Affero GNU Version 3 license.

For more detailed information, please consult the HTML documentation in
<doc/ArgyllDoc.html>, or <http://www.argyllcms.com/doc/ArgyllDoc.html>.

For the most recent source code start at <http://www.argyllcms.com/index.html>.

Contact me in regards to Argyll, icclib or cgatslib at:

	Graeme at argyllcms dot com

Enjoy!
