# About new-line characters

New-line characters (CR or CR+LF) received from the host are converted to CR+LF pairs by Tera Term, and then Tera Term sends them to MACRO.
You should use the pair (CR+LF) as a new-line character to send to Tera Term.
ASCII code 13 (decimal) is for CR, and 10 is for LF.

Example:

`send 'abc'#13#10` | Same as the statement "`sendln 'abc'`". The actual new-line character to be sent to the host is determined by Tera Term.
`wait #10'abc' 'def'#13` | Waits for a line beginning with "abc" or a line ending with "def".
`logwrite 'abc'#13#10` | Writes line "abc" to the log file.