# `.dex` — Dalvik Executable Format

Copyright © 2007 The Android Open Source Project

This document describes the layout and contents of `.dex` files, which are used to hold a set of class definitions and their associated adjunct data.

# Guide To Types

Name | Description
--- | ---
byte | 8-bit signed int
ubyte | 8-bit unsigned int
short | 16-bit signed int, little-endian
ushort | 16-bit unsigned int, little-endian
int | 32-bit signed int, little-endian
uint | 32-bit unsigned int, little-endian
long | 64-bit signed int, little-endian
ulong | 64-bit unsigned int, little-endian
sleb128 | signed LEB128, variable-length (see below)
uleb128 | unsigned LEB128, variable-length (see below)
uleb128p1 | unsigned LEB128 plus `1`, variable-length (see below)

### LEB128

LEB128 ("Little-Endian Base 128") is a variable-length encoding for arbitrary signed or unsigned integer quantities. The format was borrowed from the DWARF3 specification. In a `.dex` file, LEB128 is only ever used to encode 32-bit quantities.

Each LEB128 encoded value consists of one to five bytes, which together represent a single 32-bit value. Each byte has its most significant bit set except for the final byte in the sequence, which has its most significant bit clear. The remaining seven bits of each byte are payload, with the least significant seven bits of the quantity in the first byte, the next seven in the second byte and so on. In the case of a signed LEB128 (`sleb128`), the most significant payload bit of the final byte in the sequence is sign-extended to produce the final value. In the unsigned case (`uleb128`), any bits not explicitly represented are interpreted as `0`.

Bitwise diagram of a two-byte LEB128 value
First byte | Second byte
--- | ---
`1` | bit6 | bit5 | bit4 | bit3 | bit2 | bit1 | bit0 | `0` | bit13 | bit12 | bit11 | bit10 | bit9 | bit8 | bit7

The variant `uleb128p1` is used to represent a signed value, where the representation is of the value plus one encoded as a `uleb128`. This makes the encoding of `-1` (alternatively thought of as the unsigned value `0xffffffff`) — but no other negative number — a single byte, and is useful in exactly those cases where the represented number must either be non-negative or `-1` (or `0xffffffff`), and where no other negative values are allowed (or where large unsigned values are unlikely to be needed).

Here are some examples of the formats:

Encoded Sequence | As `sleb128` | As `uleb128` | As `uleb128p1`
--- | --- | --- | ---
00 | 0 | 0 | -1
01 | 1 | 1 | 0
7f | -1 | 127 | 126
80 7f | -128 | 16256 | 16255

# Overall File Layout

Name | Format | Description
--- | --- | ---
header | header_item | the header
string_ids | string_id_item[] | string identifiers list. These are identifiers for all the strings used by this file, either for internal naming (e.g., type descriptors) or as constant objects referred to by code. This list must be sorted by string contents, using UTF-16 code point values (not in a locale-sensitive manner).
type_ids | type_id_item[] | type identifiers list. These are identifiers for all types (classes, arrays, or primitive types) referred to by this file, whether defined in the file or not. This list must be sorted by `string_id` index.
proto_ids | proto_id_item[] | method prototype identifiers list. These are identifiers for all prototypes referred to by this file. This list must be sorted in return-type (by `type_id` index) major order, and then by arguments (also by `type_id` index).
field_ids | field_id_item[] | field identifiers list. These are identifiers for all fields referred to by this file, whether defined in the file or not. This list must be sorted, where the defining type (by `type_id` index) is the major order, field name (by `string_id` index) is the intermediate order, and type (by `type_id` index) is the minor order.
method_ids | method_id_item[] | method identifiers list. These are identifiers for all methods referred to by this file, whether defined in the file or not. This list must be sorted, where the defining type (by `type_id` index) is the major order, method name (by `string_id` index) is the intermediate order, and method prototype (by `proto_id` index) is the minor order.
class_defs | class_def_item[] | class definitions list. The classes must be ordered such that a given class's superclass and implemented interfaces appear in the list earlier than the referring class.
data | ubyte[] | data area, containing all the support data for the tables listed above. Different items have different alignment requirements, and padding bytes are inserted before each item if necessary to achieve proper alignment.
link_data | ubyte[] | data used in statically linked files. The format of the data in this section is left unspecified by this document; this section is empty in unlinked files, and runtime implementations may use it as they see fit.

# Bitfield, String, and Constant Definitions

## `DEX_FILE_MAGIC`

#### embedded in `header_item`

The constant array/string `DEX_FILE_MAGIC` is the list of bytes that must appear at the beginning of a `.dex` file in order for it to be recognized as such. The value intentionally contains a newline (`"\n"` or `0x0a`) and a null byte (`"\0"` or `0x00`) in order to help in the detection of certain forms of corruption. The value also encodes a format version number as three decimal digits, which is expected to increase monotonically over time as the format evolves.

    ubyte[8] DEX_FILE_MAGIC = { 0x64 0x65 0x78 0x0a 0x30 0x33 0x35 0x00 }
                            = "dex\n035\0"

Note: At least a couple earlier versions of the format have been used in widely-available public software releases. For example, version `009` was used for the M3 releases of the Android platform (November-December 2007), and version `013` was used for the M5 releases of the Android platform (February-March 2008). In several respects, these earlier versions of the format differ significantly from the version described in this document.

## `ENDIAN_CONSTANT` and `REVERSE_ENDIAN_CONSTANT`

#### embedded in `header_item`

The constant `ENDIAN_CONSTANT` is used to indicate the endianness of the file in which it is found. Although the standard `.dex` format is little-endian, implementations may choose to perform byte-swapping. Should an implementation come across a header whose `endian_tag` is `REVERSE_ENDIAN_CONSTANT` instead of `ENDIAN_CONSTANT`, it would know that the file has been byte-swapped from the expected form.

    uint ENDIAN_CONSTANT = 0x12345678;
    uint REVERSE_ENDIAN_CONSTANT = 0x78563412;

## `NO_INDEX`

#### embedded in `class_def_item` and `debug_info_item`

The constant `NO_INDEX` is used to indicate that an index value is absent.

Note: This value isn't defined to be `0`, because that is in fact typically a valid index.

Also Note: The chosen value for `NO_INDEX` is representable as a single byte in the `uleb128p1` encoding.

    uint NO_INDEX = 0xffffffff;    // == -1 if treated as a signed int

## `access_flags` Definitions

#### embedded in `class_def_item`, `field_item`, `method_item`, and `InnerClass`

Bitfields of these flags are used to indicate the accessibility and overall properties of classes and class members.

Name | Value | For Classes (and `InnerClass` annotations) | For Fields | For Methods
--- | --- | --- | --- | ---
ACC_PUBLIC | 0x1 | `public`: visible everywhere | `public`: visible everywhere | `public`: visible everywhere
ACC_PRIVATE | 0x2 | * `private`: only visible to defining class | `private`: only visible to defining class | `private`: only visible to defining class
ACC_PROTECTED | 0x4 | * `protected`: visible to package and subclasses | `protected`: visible to package and subclasses | `protected`: visible to package and subclasses
ACC_STATIC | 0x8 | * `static`: is not constructed with an outer `this` reference | `static`: global to defining class | `static`: does not take a `this` argument
ACC_FINAL | 0x10 | `final`: not subclassable | `final`: immutable after construction | `final`: not overridable
ACC_SYNCHRONIZED | 0x20 |  |  | `synchronized`: associated lock automatically acquired around call to this method. Note: This is only valid to set when `ACC_NATIVE` is also set.
ACC_VOLATILE | 0x40 |  | `volatile`: special access rules to help with thread safety |
ACC_BRIDGE | 0x40 |  |  | bridge method, added automatically by compiler as a type-safe bridge
ACC_TRANSIENT | 0x80 |  | `transient`: not to be saved by default serialization |
ACC_VARARGS | 0x80 |  |  | last argument should be treated as a "rest" argument by compiler
ACC_NATIVE | 0x100 |  |  | `native`: implemented in native code
ACC_INTERFACE | 0x200 | `interface`: multiply-implementable abstract class |  |
ACC_ABSTRACT | 0x400 | `abstract`: not directly instantiable |  | `abstract`: unimplemented by this class
ACC_STRICT | 0x800 |  |  | `strictfp`: strict rules for floating-point arithmetic
ACC_SYNTHETIC | 0x1000 | not directly defined in source code | not directly defined in source code | not directly defined in source code
ACC_ANNOTATION | 0x2000 | declared as an annotation class |  |
ACC_ENUM | 0x4000 | declared as an enumerated type | declared as an enumerated value |
(unused) | 0x8000 |  |  |
ACC_CONSTRUCTOR | 0x10000 |  |  | constructor method (class or instance initializer)
ACC_DECLARED_ SYNCHRONIZED | 0x20000 |  |  | declared `synchronized`. Note: This has no effect on execution (other than in reflection of this flag, per se).

* Only allowed on for `InnerClass` annotations, and must not ever be on in a `class_def_item`.

## MUTF-8 (Modified UTF-8) Encoding

As a concession to easier legacy support, the `.dex` format encodes its string data in a de facto standard modified UTF-8 form, hereafter referred to as MUTF-8. This form is identical to standard UTF-8, except:

- Only the one-, two-, and three-byte encodings are used.
- Code points in the range `U+10000` … `U+10ffff` are encoded as a surrogate pair, each of which is represented as a three-byte encoded value.
- The code point `U+0000` is encoded in two-byte form.
- A plain null byte (value `0`) indicates the end of a string, as is the standard C language interpretation.

The first two items above can be summarized as: MUTF-8 is an encoding format for UTF-16, instead of being a more direct encoding format for Unicode characters.

The final two items above make it simultaneously possible to include the code point `U+0000` in a string and still manipulate it as a C-style null-terminated string.

However, the special encoding of `U+0000` means that, unlike normal UTF-8, the result of calling the standard C function `strcmp()` on a pair of MUTF-8 strings does not always indicate the properly signed result of comparison of unequal strings. When ordering (not just equality) is a concern, the most straightforward way to compare MUTF-8 strings is to decode them character by character, and compare the decoded values. (However, more clever implementations are also possible.)

Please refer to The Unicode Standard for further information about character encoding. MUTF-8 is actually closer to the (relatively less well-known) encoding CESU-8 than to UTF-8 per se.

## `encoded_value` Encoding

#### embedded in `annotation_element` and `encoded_array_item`

An `encoded_value` is an encoded piece of (nearly) arbitrary hierarchically structured data. The encoding is meant to be both compact and straightforward to parse.

Name | Format | Description
--- | --- | ---
(value_arg << 5) | value_type | ubyte | byte indicating the type of the immediately subsequent `value` along with an optional clarifying argument in the high-order three bits. See below for the various `value` definitions. In most cases, `value_arg` encodes the length of the immediately-subsequent `value` in bytes, as `(size - 1)`, e.g., `0` means that the value requires one byte, and `7` means it requires eight bytes; however, there are exceptions as noted below.
value | ubyte[] | bytes representing the value, variable in length and interpreted differently for different `value_type` bytes, though always little-endian. See the various value definitions below for details.

### Value Formats

Type Name | `value_type` | `value_arg` Format | `value` Format | Description
--- | --- | --- | --- | ---
VALUE_BYTE | 0x00 | (none; must be `0`) | ubyte[1] | signed one-byte integer value
VALUE_SHORT | 0x02 | size - 1 (0…1) | ubyte[size] | signed two-byte integer value, sign-extended
VALUE_CHAR | 0x03 | size - 1 (0…1) | ubyte[size] | unsigned two-byte integer value, zero-extended
VALUE_INT | 0x04 | size - 1 (0…3) | ubyte[size] | signed four-byte integer value, sign-extended
VALUE_LONG | 0x06 | size - 1 (0…7) | ubyte[size] | signed eight-byte integer value, sign-extended
VALUE_FLOAT | 0x10 | size - 1 (0…3) | ubyte[size] | four-byte bit pattern, zero-extended to the right, and interpreted as an IEEE754 32-bit floating point value
VALUE_DOUBLE | 0x11 | size - 1 (0…7) | ubyte[size] | eight-byte bit pattern, zero-extended to the right, and interpreted as an IEEE754 64-bit floating point value
VALUE_STRING | 0x17 | size - 1 (0…3) | ubyte[size] | unsigned (zero-extended) four-byte integer value, interpreted as an index into the `string_ids` section and representing a string value
VALUE_TYPE | 0x18 | size - 1 (0…3) | ubyte[size] | unsigned (zero-extended) four-byte integer value, interpreted as an index into the `type_ids` section and representing a reflective type/class value
VALUE_FIELD | 0x19 | size - 1 (0…3) | ubyte[size] | unsigned (zero-extended) four-byte integer value, interpreted as an index into the `field_ids` section and representing a reflective field value
VALUE_METHOD | 0x1a | size - 1 (0…3) | ubyte[size] | unsigned (zero-extended) four-byte integer value, interpreted as an index into the `method_ids` section and representing a reflective method value
VALUE_ENUM | 0x1b | size - 1 (0…3) | ubyte[size] | unsigned (zero-extended) four-byte integer value, interpreted as an index into the `field_ids` section and representing the value of an enumerated type constant
VALUE_ARRAY | 0x1c | (none; must be `0`) | encoded_array | an array of values, in the format specified by "`encoded_array` Format" below. The size of the `value` is implicit in the encoding.
VALUE_ANNOTATION | 0x1d | (none; must be `0`) | encoded_annotation | a sub-annotation, in the format specified by "`encoded_annotation` Format" below. The size of the `value` is implicit in the encoding.
VALUE_NULL | 0x1e | (none; must be `0`) | (none) | `null` reference value
VALUE_BOOLEAN | 0x1f | boolean (0…1) | (none) | one-bit value; `0` for `false` and `1` for `true`. The bit is represented in the `value_arg`.

### `encoded_array` Format

Name | Format | Description
--- | --- | ---
size | uleb128 | number of elements in the array
values | encoded_value[size] | a series of `size` `encoded_value` byte sequences in the format specified by this section, concatenated sequentially.

### `encoded_annotation` Format

Name | Format | Description
--- | --- | ---
type_idx | uleb128 | type of the annotation. This must be a class (not array or primitive) type.
size | uleb128 | number of name-value mappings in this annotation
elements | annotation_element[size] | elements of the annotataion, represented directly in-line (not as offsets). Elements must be sorted in increasing order by `string_id` index.

### `annotation_element` Format

Name | Format | Description
--- | --- | ---
name_idx | uleb128 | element name, represented as an index into the `string_ids` section. The string must conform to the syntax for MemberName, defined above.
value | encoded_value | element value

## String Syntax

There are several kinds of item in a `.dex` file which ultimately refer to a string. The following BNF-style definitions indicate the acceptable syntax for these strings.

### SimpleName

A SimpleName is the basis for the syntax of the names of other things. The `.dex` format allows a fair amount of latitude here (much more than most common source languages). In brief, a simple name may consist of any low-ASCII alphabetic character or digit, a few specific low-ASCII symbols, and most non-ASCII code points that are not control, space, or special characters. Note that surrogate code points (in the range `U+d800` … `U+dfff`) are not considered valid name characters, per se, but Unicode supplemental characters are valid (which are represented by the final alternative of the rule for SimpleNameChar), and they should be represented in a file as pairs of surrogate code points in the MUTF-8 encoding.

SimpleName →
| SimpleNameChar (SimpleNameChar)*
SimpleNameChar →
| `'A'` … `'Z'`
| | `'a'` … `'z'`
| | `'0'` … `'9'`
| | `'$'`
| | `'-'`
| | `'_'`
| | `U+00a1` … `U+1fff`
| | `U+2010` … `U+2027`
| | `U+2030` … `U+d7ff`
| | `U+e000` … `U+ffef`
| | `U+10000` … `U+10ffff`

### MemberName

#### used by `field_id_item` and `method_id_item`

A MemberName is the name of a member of a class, members being fields, methods, and inner classes.

MemberName →
| SimpleName
| | `'<'` SimpleName `'>'`

### FullClassName

A FullClassName is a fully-qualified class name, including an optional package specifier followed by a required name.

FullClassName →
| OptionalPackagePrefix SimpleName
OptionalPackagePrefix →
| (SimpleName `'/'`)*

### TypeDescriptor

#### used by `type_id_item`

A TypeDescriptor is the representation of any type, including primitives, classes, arrays, and `void`. See below for the meaning of the various versions.

TypeDescriptor →
| `'V'`
| | FieldTypeDescriptor
FieldTypeDescriptor →
| NonArrayFieldTypeDescriptor
| | (`'['` * 1…255) NonArrayFieldTypeDescriptor
NonArrayFieldTypeDescriptor→
| `'Z'`
| | `'B'`
| | `'S'`
| | `'C'`
| | `'I'`
| | `'J'`
| | `'F'`
| | `'D'`
| | `'L'` FullClassName `';'`

### ShortyDescriptor

#### used by `proto_id_item`

A ShortyDescriptor is the short form representation of a method prototype, including return and parameter types, except that there is no distinction between various reference (class or array) types. Instead, all reference types are represented by a single `'L'` character.

ShortyDescriptor →
| ShortyReturnType (ShortyFieldType)*
ShortyReturnType →
| `'V'`
| | ShortyFieldType
ShortyFieldType →
| `'Z'`
| | `'B'`
| | `'S'`
| | `'C'`
| | `'I'`
| | `'J'`
| | `'F'`
| | `'D'`
| | `'L'`

## TypeDescriptor Semantics

This is the meaning of each of the variants of TypeDescriptor.

Syntax | Meaning
--- | ---
V | `void`; only valid for return types
Z | `boolean`
B | `byte`
S | `short`
C | `char`
I | `int`
J | `long`
F | `float`
D | `double`
Lfully/qualified/Name; | the class `fully.qualified.Name`
[descriptor | array of `descriptor`, usable recursively for arrays-of-arrays, though it is invalid to have more than 255 dimensions.

# Items and Related Structures

This section includes definitions for each of the top-level items that may appear in a `.dex` file.

## `header_item`

#### appears in the `header` section

#### alignment: 4 bytes

Name | Format | Description
--- | --- | ---
magic | ubyte[8] = DEX_FILE_MAGIC | magic value. See discussion above under "`DEX_FILE_MAGIC`" for more details.
checksum | uint | adler32 checksum of the rest of the file (everything but `magic` and this field); used to detect file corruption
signature | ubyte[20] | SHA-1 signature (hash) of the rest of the file (everything but `magic`, `checksum`, and this field); used to uniquely identify files
file_size | uint | size of the entire file (including the header), in bytes
header_size | uint = 0x70 | size of the header (this entire section), in bytes. This allows for at least a limited amount of backwards/forwards compatibility without invalidating the format.
endian_tag | uint = ENDIAN_CONSTANT | endianness tag. See discussion above under "`ENDIAN_CONSTANT` and `REVERSE_ENDIAN_CONSTANT`" for more details.
link_size | uint | size of the link section, or `0` if this file isn't statically linked
link_off | uint | offset from the start of the file to the link section, or `0` if `link_size == 0`. The offset, if non-zero, should be to an offset into the `link_data` section. The format of the data pointed at is left unspecified by this document; this header field (and the previous) are left as hooks for use by runtime implementations.
map_off | uint | offset from the start of the file to the map item, or `0` if this file has no map. The offset, if non-zero, should be to an offset into the `data` section, and the data should be in the format specified by "`map_list`" below.
string_ids_size | uint | count of strings in the string identifiers list
string_ids_off | uint | offset from the start of the file to the string identifiers list, or `0` if `string_ids_size == 0` (admittedly a strange edge case). The offset, if non-zero, should be to the start of the `string_ids` section.
type_ids_size | uint | count of elements in the type identifiers list
type_ids_off | uint | offset from the start of the file to the type identifiers list, or `0` if `type_ids_size == 0` (admittedly a strange edge case). The offset, if non-zero, should be to the start of the `type_ids` section.
proto_ids_size | uint | count of elements in the prototype identifiers list
proto_ids_off | uint | offset from the start of the file to the prototype identifiers list, or `0` if `proto_ids_size == 0` (admittedly a strange edge case). The offset, if non-zero, should be to the start of the `proto_ids` section.
field_ids_size | uint | count of elements in the field identifiers list
field_ids_off | uint | offset from the start of the file to the field identifiers list, or `0` if `field_ids_size == 0`. The offset, if non-zero, should be to the start of the `field_ids` section.
method_ids_size | uint | count of elements in the method identifiers list
method_ids_off | uint | offset from the start of the file to the method identifiers list, or `0` if `method_ids_size == 0`. The offset, if non-zero, should be to the start of the `method_ids` section.
class_defs_size | uint | count of elements in the class definitions list
class_defs_off | uint | offset from the start of the file to the class definitions list, or `0` if `class_defs_size == 0` (admittedly a strange edge case). The offset, if non-zero, should be to the start of the `class_defs` section.
data_size | uint | Size of `data` section in bytes. Must be an even multiple of sizeof(uint).
data_off | uint | offset from the start of the file to the start of the `data` section.

## `map_list`

#### appears in the `data` section

#### referenced from `header_item`

#### alignment: 4 bytes

This is a list of the entire contents of a file, in order. It contains some redundancy with respect to the `header_item` but is intended to be an easy form to use to iterate over an entire file. A given type may appear at most once in a map, but there is no restriction on what order types may appear in, other than the restrictions implied by the rest of the format (e.g., a `header` section must appear first, followed by a `string_ids` section, etc.). Additionally, the map entries must be ordered by initial offset and must not overlap.

Name | Format | Description
--- | --- | ---
size | uint | size of the list, in entries
list | map_item[size] | elements of the list

### `map_item` Format

Name | Format | Description
--- | --- | ---
type | ushort | type of the items; see table below
unused | ushort | (unused)
size | uint | count of the number of items to be found at the indicated offset
offset | uint | offset from the start of the file to the items in question

### Type Codes

Item Type | Constant | Value | Item Size In Bytes
--- | --- | --- | ---
header_item | TYPE_HEADER_ITEM | 0x0000 | 0x70
string_id_item | TYPE_STRING_ID_ITEM | 0x0001 | 0x04
type_id_item | TYPE_TYPE_ID_ITEM | 0x0002 | 0x04
proto_id_item | TYPE_PROTO_ID_ITEM | 0x0003 | 0x0c
field_id_item | TYPE_FIELD_ID_ITEM | 0x0004 | 0x08
method_id_item | TYPE_METHOD_ID_ITEM | 0x0005 | 0x08
class_def_item | TYPE_CLASS_DEF_ITEM | 0x0006 | 0x20
map_list | TYPE_MAP_LIST | 0x1000 | 4 + (item.size * 12)
type_list | TYPE_TYPE_LIST | 0x1001 | 4 + (item.size * 2)
annotation_set_ref_list | TYPE_ANNOTATION_SET_REF_LIST | 0x1002 | 4 + (item.size * 4)
annotation_set_item | TYPE_ANNOTATION_SET_ITEM | 0x1003 | 4 + (item.size * 4)
class_data_item | TYPE_CLASS_DATA_ITEM | 0x2000 | implicit; must parse
code_item | TYPE_CODE_ITEM | 0x2001 | implicit; must parse
string_data_item | TYPE_STRING_DATA_ITEM | 0x2002 | implicit; must parse
debug_info_item | TYPE_DEBUG_INFO_ITEM | 0x2003 | implicit; must parse
annotation_item | TYPE_ANNOTATION_ITEM | 0x2004 | implicit; must parse
encoded_array_item | TYPE_ENCODED_ARRAY_ITEM | 0x2005 | implicit; must parse
annotations_directory_item | TYPE_ANNOTATIONS_DIRECTORY_ITEM | 0x2006 | implicit; must parse

## `string_id_item`

#### appears in the `string_ids` section

#### alignment: 4 bytes

Name | Format | Description
--- | --- | ---
string_data_off | uint | offset from the start of the file to the string data for this item. The offset should be to a location in the `data` section, and the data should be in the format specified by "`string_data_item`" below. There is no alignment requirement for the offset.

## `string_data_item`

#### appears in the `data` section

#### alignment: none (byte-aligned)

Name | Format | Description
--- | --- | ---
utf16_size | uleb128 | size of this string, in UTF-16 code units (which is the "string length" in many systems). That is, this is the decoded length of the string. (The encoded length is implied by the position of the `0` byte.)
data | ubyte[] | a series of MUTF-8 code units (a.k.a. octets, a.k.a. bytes) followed by a byte of value `0`. See "MUTF-8 (Modified UTF-8) Encoding" above for details and discussion about the data format. Note: It is acceptable to have a string which includes (the encoded form of) UTF-16 surrogate code units (that is, `U+d800` … `U+dfff`) either in isolation or out-of-order with respect to the usual encoding of Unicode into UTF-16. It is up to higher-level uses of strings to reject such invalid encodings, if appropriate.

## `type_id_item`

#### appears in the `type_ids` section

#### alignment: 4 bytes

Name | Format | Description
--- | --- | ---
descriptor_idx | uint | index into the `string_ids` list for the descriptor string of this type. The string must conform to the syntax for TypeDescriptor, defined above.

## `proto_id_item`

#### appears in the `proto_ids` section

#### alignment: 4 bytes

Name | Format | Description
--- | --- | ---
shorty_idx | uint | index into the `string_ids` list for the short-form descriptor string of this prototype. The string must conform to the syntax for ShortyDescriptor, defined above, and must correspond to the return type and parameters of this item.
return_type_idx | uint | index into the `type_ids` list for the return type of this prototype
parameters_off | uint | offset from the start of the file to the list of parameter types for this prototype, or `0` if this prototype has no parameters. This offset, if non-zero, should be in the `data` section, and the data there should be in the format specified by `"type_list"` below. Additionally, there should be no reference to the type `void` in the list.

## `field_id_item`

#### appears in the `field_ids` section

#### alignment: 4 bytes

Name | Format | Description
--- | --- | ---
class_idx | ushort | index into the `type_ids` list for the definer of this field. This must be a class type, and not an array or primitive type.
type_idx | ushort | index into the `type_ids` list for the type of this field
name_idx | uint | index into the `string_ids` list for the name of this field. The string must conform to the syntax for MemberName, defined above.

## `method_id_item`

#### appears in the `method_ids` section

#### alignment: 4 bytes

Name | Format | Description
--- | --- | ---
class_idx | ushort | index into the `type_ids` list for the definer of this method. This must be a class or array type, and not a primitive type.
proto_idx | ushort | index into the `proto_ids` list for the prototype of this method
name_idx | uint | index into the `string_ids` list for the name of this method. The string must conform to the syntax for MemberName, defined above.

## `class_def_item`

#### appears in the `class_defs` section

#### alignment: 4 bytes

Name | Format | Description
--- | --- | ---
class_idx | uint | index into the `type_ids` list for this class. This must be a class type, and not an array or primitive type.
access_flags | uint | access flags for the class (`public`, `final`, etc.). See "`access_flags` Definitions" for details.
superclass_idx | uint | index into the `type_ids` list for the superclass, or the constant value `NO_INDEX` if this class has no superclass (i.e., it is a root class such as `Object`). If present, this must be a class type, and not an array or primitive type.
interfaces_off | uint | offset from the start of the file to the list of interfaces, or `0` if there are none. This offset should be in the `data` section, and the data there should be in the format specified by "`type_list`" below. Each of the elements of the list must be a class type (not an array or primitive type), and there must not be any duplicates.
source_file_idx | uint | index into the `string_ids` list for the name of the file containing the original source for (at least most of) this class, or the special value `NO_INDEX` to represent a lack of this information. The `debug_info_item` of any given method may override this source file, but the expectation is that most classes will only come from one source file.
annotations_off | uint | offset from the start of the file to the annotations structure for this class, or `0` if there are no annotations on this class. This offset, if non-zero, should be in the `data` section, and the data there should be in the format specified by "`annotations_directory_item`" below, with all items referring to this class as the definer.
class_data_off | uint | offset from the start of the file to the associated class data for this item, or `0` if there is no class data for this class. (This may be the case, for example, if this class is a marker interface.) The offset, if non-zero, should be in the `data` section, and the data there should be in the format specified by "`class_data_item`" below, with all items referring to this class as the definer.
static_values_off | uint | offset from the start of the file to the list of initial values for `static` fields, or `0` if there are none (and all `static` fields are to be initialized with `0` or `null`). This offset should be in the `data` section, and the data there should be in the format specified by "`encoded_array_item`" below. The size of the array must be no larger than the number of `static` fields declared by this class, and the elements correspond to the `static` fields in the same order as declared in the corresponding `field_list`. The type of each array element must match the declared type of its corresponding field. If there are fewer elements in the array than there are `static` fields, then the leftover fields are initialized with a type-appropriate `0` or `null`.

## `class_data_item`

#### referenced from `class_def_item`

#### appears in the `data` section

#### alignment: none (byte-aligned)

Name | Format | Description
--- | --- | ---
static_fields_size | uleb128 | the number of static fields defined in this item
instance_fields_size | uleb128 | the number of instance fields defined in this item
direct_methods_size | uleb128 | the number of direct methods defined in this item
virtual_methods_size | uleb128 | the number of virtual methods defined in this item
static_fields | encoded_field[static_fields_size] | the defined static fields, represented as a sequence of encoded elements. The fields must be sorted by `field_idx` in increasing order.
instance_fields | encoded_field[instance_fields_size] | the defined instance fields, represented as a sequence of encoded elements. The fields must be sorted by `field_idx` in increasing order.
direct_methods | encoded_method[direct_methods_size] | the defined direct (any of `static`, `private`, or constructor) methods, represented as a sequence of encoded elements. The methods must be sorted by `method_idx` in increasing order.
virtual_methods | encoded_method[virtual_methods_size] | the defined virtual (none of `static`, `private`, or constructor) methods, represented as a sequence of encoded elements. This list should not include inherited methods unless overridden by the class that this item represents. The methods must be sorted by `method_idx` in increasing order.

Note: All elements' `field_id`s and `method_id`s must refer to the same defining class.

### `encoded_field` Format

Name | Format | Description
--- | --- | ---
field_idx_diff | uleb128 | index into the `field_ids` list for the identity of this field (includes the name and descriptor), represented as a difference from the index of previous element in the list. The index of the first element in a list is represented directly.
access_flags | uleb128 | access flags for the field (`public`, `final`, etc.). See "`access_flags` Definitions" for details.

### `encoded_method` Format

Name | Format | Description
--- | --- | ---
method_idx_diff | uleb128 | index into the `method_ids` list for the identity of this method (includes the name and descriptor), represented as a difference from the index of previous element in the list. The index of the first element in a list is represented directly.
access_flags | uleb128 | access flags for the method (`public`, `final`, etc.). See "`access_flags` Definitions" for details.
code_off | uleb128 | offset from the start of the file to the code structure for this method, or `0` if this method is either `abstract` or `native`. The offset should be to a location in the `data` section. The format of the data is specified by "`code_item`" below.

## `type_list`

#### referenced from `class_def_item` and `proto_id_item`

#### appears in the `data` section

#### alignment: 4 bytes

Name | Format | Description
--- | --- | ---
size | uint | size of the list, in entries
list | type_item[size] | elements of the list

### `type_item` Format

Name | Format | Description
--- | --- | ---
type_idx | ushort | index into the `type_ids` list

## `code_item`

#### referenced from `method_item`

#### appears in the `data` section

#### alignment: 4 bytes

Name | Format | Description
--- | --- | ---
registers_size | ushort | the number of registers used by this code
ins_size | ushort | the number of words of incoming arguments to the method that this code is for
outs_size | ushort | the number of words of outgoing argument space required by this code for method invocation
tries_size | ushort | the number of `try_item`s for this instance. If non-zero, then these appear as the `tries` array just after the `insns` in this instance.
debug_info_off | uint | offset from the start of the file to the debug info (line numbers + local variable info) sequence for this code, or `0` if there simply is no information. The offset, if non-zero, should be to a location in the `data` section. The format of the data is specified by "`debug_info_item`" below.
insns_size | uint | size of the instructions list, in 16-bit code units
insns | ushort[insns_size] | actual array of bytecode. The format of code in an `insns` array is specified by the companion document "Bytecode for the Dalvik VM". Note that though this is defined as an array of `ushort`, there are some internal structures that prefer four-byte alignment. Also, if this happens to be in an endian-swapped file, then the swapping is only done on individual `ushort`s and not on the larger internal structures.
padding | ushort (optional) = 0 | two bytes of padding to make `tries` four-byte aligned. This element is only present if `tries_size` is non-zero and `insns_size` is odd.
tries | try_item[tries_size] (optional) | array indicating where in the code exceptions may be caught and how to handle them. Elements of the array must be non-overlapping in range and in order from low to high address. This element is only present if `tries_size` is non-zero.
handlers | encoded_catch_handler_list (optional) | bytes representing a list of lists of catch types and associated handler addresses. Each `try_item` has a byte-wise offset into this structure. This element is only present if `tries_size` is non-zero.

### `try_item` Format

Name | Format | Description
--- | --- | ---
start_addr | uint | start address of the block of code covered by this entry. The address is a count of 16-bit code units to the start of the first covered instruction.
insn_count | ushort | number of 16-bit code units covered by this entry. The last code unit covered (inclusive) is `start_addr + insn_count - 1`.
handler_off | ushort | offset in bytes from the start of the associated encoded handler data to the `catch_handler_item` for this entry

### `encoded_catch_handler_list` Format

Name | Format | Description
--- | --- | ---
size | uleb128 | size of this list, in entries
list | encoded_catch_handler[handlers_size] | actual list of handler lists, represented directly (not as offsets), and concatenated sequentially

### `encoded_catch_handler` Format

Name | Format | Description
--- | --- | ---
size | sleb128 | number of catch types in this list. If non-positive, then this is the negative of the number of catch types, and the catches are followed by a catch-all handler. For example: A `size` of `0` means that there is a catch-all but no explicitly typed catches. A `size` of `2` means that there are two explicitly typed catches and no catch-all. And a `size` of `-1` means that there is one typed catch along with a catch-all.
handlers | encoded_type_addr_pair[abs(size)] | stream of `abs(size)` encoded items, one for each caught type, in the order that the types should be tested.
catch_all_addr | uleb128 (optional) | bytecode address of the catch-all handler. This element is only present if `size` is non-positive.

### `encoded_type_addr_pair` Format

Name | Format | Description
--- | --- | ---
type_idx | uleb128 | index into the `type_ids` list for the type of the exception to catch
addr | uleb128 | bytecode address of the associated exception handler

## `debug_info_item`

#### referenced from `code_item`

#### appears in the `data` section

#### alignment: none (byte-aligned)

Each `debug_info_item` defines a DWARF3-inspired byte-coded state machine that, when interpreted, emits the positions table and (potentially) the local variable information for a `code_item`. The sequence begins with a variable-length header (the length of which depends on the number of method parameters), is followed by the state machine bytecodes, and ends with an `DBG_END_SEQUENCE` byte.

The state machine consists of five registers. The `address` register represents the instruction offset in the associated `insns_item` in 16-bit code units. The `address` register starts at `0` at the beginning of each `debug_info` sequence and may only monotonically increase. The `line` register represents what source line number should be associated with the next positions table entry emitted by the state machine. It is initialized in the sequence header, and may change in positive or negative directions but must never be less than `1`. The `source_file` register represents the source file that the line number entries refer to. It is initialized to the value of `source_file_idx` in `class_def_item`. The other two variables, `prologue_end` and `epilogue_begin`, are boolean flags (initialized to `false`) that indicate whether the next position emitted should be considered a method prologue or epilogue. The state machine must also track the name and type of the last local variable live in each register for the `DBG_RESTART_LOCAL` code.

The header is as follows:

Name | Format | Description
--- | --- | ---
line_start | uleb128 | the initial value for the state machine's `line` register. Does not represent an actual positions entry.
parameters_size | uleb128 | the number of parameter names that are encoded. There should be one per method parameter, excluding an instance method's `this`, if any.
parameter_names | uleb128p1[parameters_size] | string index of the method parameter name. An encoded value of `NO_INDEX` indicates that no name is available for the associated parameter. The type descriptor and signature are implied from the method descriptor and signature.

The byte code values are as follows:

Name | Value | Format | Arguments | Description
--- | --- | --- | --- | ---
DBG_END_SEQUENCE | 0x00 |  | (none) | terminates a debug info sequence for a `code_item`
DBG_ADVANCE_PC | 0x01 | uleb128 addr_diff | `addr_diff`: amount to add to address register | advances the address register without emitting a positions entry
DBG_ADVANCE_LINE | 0x02 | sleb128 line_diff | `line_diff`: amount to change line register by | advances the line register without emitting a positions entry
DBG_START_LOCAL | 0x03 | uleb128 register_num uleb128p1 name_idx uleb128p1 type_idx | `register_num`: register that will contain local `name_idx`: string index of the name `type_idx`: type index of the type | introduces a local variable at the current address. Either `name_idx` or `type_idx` may be `NO_INDEX` to indicate that that value is unknown.
DBG_START_LOCAL_EXTENDED | 0x04 | uleb128 register_num uleb128p1 name_idx uleb128p1 type_idx uleb128p1 sig_idx | `register_num`: register that will contain local `name_idx`: string index of the name `type_idx`: type index of the type `sig_idx`: string index of the type signature | introduces a local with a type signature at the current address. Any of `name_idx`, `type_idx`, or `sig_idx` may be `NO_INDEX` to indicate that that value is unknown. (If `sig_idx` is `-1`, though, the same data could be represented more efficiently using the opcode `DBG_START_LOCAL`.) Note: See the discussion under "`dalvik.annotation.Signature`" below for caveats about handling signatures.
DBG_END_LOCAL | 0x05 | uleb128 register_num | `register_num`: register that contained local | marks a currently-live local variable as out of scope at the current address
DBG_RESTART_LOCAL | 0x06 | uleb128 register_num | `register_num`: register to restart | re-introduces a local variable at the current address. The name and type are the same as the last local that was live in the specified register.
DBG_SET_PROLOGUE_END | 0x07 |  | (none) | sets the `prologue_end` state machine register, indicating that the next position entry that is added should be considered the end of a method prologue (an appropriate place for a method breakpoint). The `prologue_end` register is cleared by any special (`>= 0x0a`) opcode.
DBG_SET_EPILOGUE_BEGIN | 0x08 |  | (none) | sets the `epilogue_begin` state machine register, indicating that the next position entry that is added should be considered the beginning of a method epilogue (an appropriate place to suspend execution before method exit). The `epilogue_begin` register is cleared by any special (`>= 0x0a`) opcode.
DBG_SET_FILE | 0x09 | uleb128p1 name_idx | `name_idx`: string index of source file name; `NO_INDEX` if unknown | indicates that all subsequent line number entries make reference to this source file name, instead of the default name specified in `code_item`
Special Opcodes | 0x0a…0xff |  | (none) | advances the `line` and `address` registers, emits a position entry, and clears `prologue_end` and `epilogue_begin`. See below for description.

### Special Opcodes

Opcodes with values between `0x0a` and `0xff` (inclusive) move both the `line` and `address` registers by a small amount and then emit a new position table entry. The formula for the increments are as follows:

    DBG_FIRST_SPECIAL = 0x0a  // the smallest special opcode
    DBG_LINE_BASE   = -4      // the smallest line number increment
    DBG_LINE_RANGE  = 15      // the number of line increments represented

    adjusted_opcode = opcode - DBG_FIRST_SPECIAL

    line += DBG_LINE_BASE + (adjusted_opcode % DBG_LINE_RANGE)
    address += (adjusted_opcode / DBG_LINE_RANGE)

## `annotations_directory_item`

#### referenced from `class_def_item`

#### appears in the `data` section

#### alignment: 4 bytes

Name | Format | Description
--- | --- | ---
class_annotations_off | uint | offset from the start of the file to the annotations made directly on the class, or `0` if the class has no direct annotations. The offset, if non-zero, should be to a location in the `data` section. The format of the data is specified by "`annotation_set_item`" below.
fields_size | uint | count of fields annotated by this item
annotated_methods_size | uint | count of methods annotated by this item
annotated_parameters_size | uint | count of method parameter lists annotated by this item
field_annotations | field_annotation[fields_size] (optional) | list of associated field annotations. The elements of the list must be sorted in increasing order, by `field_idx`.
method_annotations | method_annotation[methods_size] (optional) | list of associated method annotations. The elements of the list must be sorted in increasing order, by `method_idx`.
parameter_annotations | parameter_annotation[parameters_size] (optional) | list of associated method parameter annotations. The elements of the list must be sorted in increasing order, by `method_idx`.

Note: All elements' `field_id`s and `method_id`s must refer to the same defining class.

### `field_annotation` Format

Name | Format | Description
--- | --- | ---
field_idx | uint | index into the `field_ids` list for the identity of the field being annotated
annotations_off | uint | offset from the start of the file to the list of annotations for the field. The offset should be to a location in the `data` section. The format of the data is specified by "`annotation_set_item`" below.

### `method_annotation` Format

Name | Format | Description
--- | --- | ---
method_idx | uint | index into the `method_ids` list for the identity of the method being annotated
annotations_off | uint | offset from the start of the file to the list of annotations for the method. The offset should be to a location in the `data` section. The format of the data is specified by "`annotation_set_item`" below.

### `parameter_annotation` Format

Name | Format | Description
--- | --- | ---
method_idx | uint | index into the `method_ids` list for the identity of the method whose parameters are being annotated
annotations_off | uint | offset from the start of the file to the list of annotations for the method parameters. The offset should be to a location in the `data` section. The format of the data is specified by "`annotation_set_ref_list`" below.

## `annotation_set_ref_list`

#### referenced from `parameter_annotations_item`

#### appears in the `data` section

#### alignment: 4 bytes

Name | Format | Description
--- | --- | ---
size | uint | size of the list, in entries
list | annotation_set_ref_item[size] | elements of the list

### `annotation_set_ref_item` Format

Name | Format | Description
--- | --- | ---
annotations_off | uint | offset from the start of the file to the referenced annotation set or `0` if there are no annotations for this element. The offset, if non-zero, should be to a location in the `data` section. The format of the data is specified by "`annotation_set_item`" below.

## `annotation_set_item`

#### referenced from `annotations_directory_item`, `field_annotations_item`, `method_annotations_item`, and `annotation_set_ref_item`

#### appears in the `data` section

#### alignment: 4 bytes

Name | Format | Description
--- | --- | ---
size | uint | size of the set, in entries
entries | annotation_off_item[size] | elements of the set. The elements must be sorted in increasing order, by `type_idx`.

### `annotation_off_item` Format

Name | Format | Description
--- | --- | ---
annotation_off | uint | offset from the start of the file to an annotation. The offset should be to a location in the `data` section, and the format of the data at that location is specified by "`annotation_item`" below.

## `annotation_item`

#### referenced from `annotation_set_item`

#### appears in the `data` section

#### alignment: none (byte-aligned)

Name | Format | Description
--- | --- | ---
visibility | ubyte | intended visibility of this annotation (see below)
annotation | encoded_annotation | encoded annotation contents, in the format described by "`encoded_annotation` Format" under "`encoded_value` Encoding" above.

### Visibility values

These are the options for the `visibility` field in an `annotation_item`:

Name | Value | Description
--- | --- | ---
VISIBILITY_BUILD | 0x00 | intended only to be visible at build time (e.g., during compilation of other code)
VISIBILITY_RUNTIME | 0x01 | intended to visible at runtime
VISIBILITY_SYSTEM | 0x02 | intended to visible at runtime, but only to the underlying system (and not to regular user code)

## `encoded_array_item`

#### referenced from `class_def_item`

#### appears in the `data` section

#### alignment: none (byte-aligned)

Name | Format | Description
--- | --- | ---
value | encoded_array | bytes representing the encoded array value, in the format specified by "`encoded_array` Format" under "`encoded_value` Encoding" above.

# System Annotations

System annotations are used to represent various pieces of reflective information about classes (and methods and fields). This information is generally only accessed indirectly by client (non-system) code.

System annotations are represented in `.dex` files as annotations with visibility set to `VISIBILITY_SYSTEM`.

## `dalvik.annotation.AnnotationDefault`

#### appears on methods in annotation interfaces

An `AnnotationDefault` annotation is attached to each annotation interface which wishes to indicate default bindings.

Name | Format | Description
--- | --- | ---
value | Annotation | the default bindings for this annotation, represented as an annotation of this type. The annotation need not include all names defined by the annotation; missing names simply do not have defaults.

## `dalvik.annotation.EnclosingClass`

#### appears on classes

An `EnclosingClass` annotation is attached to each class which is either defined as a member of another class, per se, or is anonymous but not defined within a method body (e.g., a synthetic inner class). Every class that has this annotation must also have an `InnerClass` annotation. Additionally, a class may not have both an `EnclosingClass` and an `EnclosingMethod` annotation.

Name | Format | Description
--- | --- | ---
value | Class | the class which most closely lexically scopes this class

## `dalvik.annotation.EnclosingMethod`

#### appears on classes

An `EnclosingMethod` annotation is attached to each class which is defined inside a method body. Every class that has this annotation must also have an `InnerClass` annotation. Additionally, a class may not have both an `EnclosingClass` and an `EnclosingMethod` annotation.

Name | Format | Description
--- | --- | ---
value | Method | the method which most closely lexically scopes this class

## `dalvik.annotation.InnerClass`

#### appears on classes

An `InnerClass` annotation is attached to each class which is defined in the lexical scope of another class's definition. Any class which has this annotation must also have either an `EnclosingClass` annotation or an `EnclosingMethod` annotation.

Name | Format | Description
--- | --- | ---
name | String | the originally declared simple name of this class (not including any package prefix). If this class is anonymous, then the name is `null`.
accessFlags | int | the originally declared access flags of the class (which may differ from the effective flags because of a mismatch between the execution models of the source language and target virtual machine)

## `dalvik.annotation.MemberClasses`

#### appears on classes

A `MemberClasses` annotation is attached to each class which declares member classes. (A member class is a direct inner class that has a name.)

Name | Format | Description
--- | --- | ---
value | Class[] | array of the member classes

## `dalvik.annotation.Signature`

#### appears on classes, fields, and methods

A `Signature` annotation is attached to each class, field, or method which is defined in terms of a more complicated type than is representable by a `type_id_item`. The `.dex` format does not define the format for signatures; it is merely meant to be able to represent whatever signatures a source language requires for successful implementation of that language's semantics. As such, signatures are not generally parsed (or verified) by virtual machine implementations. The signatures simply get handed off to higher-level APIs and tools (such as debuggers). Any use of a signature, therefore, should be written so as not to make any assumptions about only receiving valid signatures, explicitly guarding itself against the possibility of coming across a syntactically invalid signature.

Because signature strings tend to have a lot of duplicated content, a `Signature` annotation is defined as an array of strings, where duplicated elements naturally refer to the same underlying data, and the signature is taken to be the concatenation of all the strings in the array. There are no rules about how to pull apart a signature into separate strings; that is entirely up to the tools that generate `.dex` files.

Name | Format | Description
--- | --- | ---
value | String[] | the signature of this class or member, as an array of strings that is to be concatenated together

## `dalvik.annotation.Throws`

#### appears on methods

A `Throws` annotation is attached to each method which is declared to throw one or more exception types.

Name | Format | Description
--- | --- | ---
value | Class[] | the array of exception types thrown