
  intel-vaapi-driver
  VA driver for Intel G45 & HD Graphics family

  Copyright (C) 2009-2017 Intel Corporation


License
-------

Please read the COPYING file available in this package.


Overview
--------

intel-vaapi-driver is the VA-API implementation for Intel G45 chipsets
and Intel HD Graphics for Intel Core processor family.

Platform definitions:
CTG: Cantiga, Intel GMA 4500MHD (GM45)
ILK: Ironlake, Intel HD Graphics for 2010 Intel Core processor family
SNB: Sandybridge, Intel HD Graphics for 2011 Intel Core processor family
IVB: Ivybridge
HSW: Haswell
BDW: Broadwell
CHV/BSW: Cherryview/Braswell
SKL: Skylake
BXT: Broxton
KBL: Kabylake

Codecs
------

H.264   D   ILK+
H.264   E   SNB+
MPEG-2  D   CTG+
VC-1    D   SNB+
JPEG    D   IVB+
JPEG    E   CHV+/BSW+
VP8     D   BDW+
VP8     E   CHV+/BSW+
HEVC    D   CHV+/BSW+
HEVC    E   SKL+
VP9     D   BXT+
VP9     E   KBL+
HEVC 10bit     D       BXT+
HEVC 10bit     E       KBL+
VP9 10bit      D       KBL+

Requirements
------------

libva >= 1.7.0

Testing
-------

Please read the TESTING file available in this package.
